Total N (TN) and total P (TP) loads for large river systems in NC were calculated at locations as close as possible to the heads of estuaries based on USGS gaged river flows (see metadata for river flows) and nutrient concentrations measured by the NC Div. of Water Resources Ambient Monitoring Program. Stations where nutrient concentration data were gathered is shown in Table 1 below. Loads were calculated from daily mean flow and approximately monthly concentration data using the USGS regression model, weighted regressions on time, discharge and season (WRTDS) (Hirsh et al. 2010). TN was calculated as the sum of total Kjeldhal nitrogen and nitrate/nitrite. An example script used to sum the total Kjeldhal nitrogen and nitrate/nitrite values for each observation date is provided on Github in the scripts folder. For the WRTDS load modeling, a half window width of seven years and minimum number of observations of 50 were used. An example script for calculating TP loads for the Neuse River at Streets Ferry Bridge is included on Github in the scripts folder. Otherwise, all other model parameters were left at their default values and can be provided in Hirsch et al. (2015). Model estimates of daily TN and TP loads were summed by year and by seasons within years to produce annual time series of loads for the whole year and by season. Example code for summing the WRTDS daily estimates by year and season is provided on Github in the scripts folder.

|  |  |  |
| --- | --- | --- |
| Table 1. North Carolina Division of Water Resources Ambient Monitoring Program stations where TN and TP data were measured to calculate TN and TP loads | | |
| River | NC DWR Ambient Monitoring Program Station | Time span |
| Cape Fear River | B8350000 above Lock and Dam 1 | 1974-2019 |
| Neuse River | J7930000 at Streets Ferry Bridge | 1974-2019 |
| Tar River | 05250000 at Tarboro | 1974-2019 |
| Roanoke River | N9250000 near Plymouth | 1974-2019 |
| Chowan River | D0010000 near Riddicksville | 1974-2019 |

Hirsch, R.M., and De Cicco, L.A., 2015, User guide to Exploration and Graphics for RivEr Trends (EGRET) and dataRetrieval—R packages for hydrologic data (version 2.0, February 2015): U.S. Geological Survey Techniques and Methods book 4, chap. A10, 93 p., [*http://dx.doi.org/10.3133/tm4A10*](http://dx.doi.org/10.3133/tm4A10)*.*

Hirsch, R.M., D.L. Moyer, and S.A. Archfield, 2010. Weighted regressions on time, discharge, and season (WRTDS), With an application to Chesapeake Bay river inputs. *Journal of the American Water Resources Association* 46:857-880.